                - - - - - CLEANING PAPER - - - - -

For details, refer to the Maintenance Chapter in your printer manual

Procedure : (Do every time EP-L cartridge is replaced) 1. If optional paper cassette is installed, tray selection must be ‘MP TRAY’. 2. Place this page, this side up, on the top of the paper stack in the MP tray. 3. Run another test page. (Cleaning once is sufficient)